Product

# Cloud PLC - RPI - 0

The Programmable Cloud PLC® offers Unmatched adaptability, reliable connectivity and customisable solution for your industry. Cloud PLC® can be utilized as an edge gateway, Automation tool, data logger & edge processing node. Cloud PLC supporting wide range of industrial protocols like Modbus, MQTT, JSON, RESTful, TCP/UDP, SNMP, OPC which makes the solution integration easier than ever for IT / Automation engineers.

### Features

- 12x Isolated Analog Input Channel 0-10V, 0-24v, 4-20mA. 16 Bit Resolution and 860SPS.
- 4x Isolated Digital Input 24V.
- 3x Isolated Digital Output / PWM 24V.
- 1x Relay (NO & C).
- 1x Isolated RS485 for MODBUS RTU Communication.
- 1x USB-Device Interface for Configuring, Monitoring & Download.
- 1x WiFi & Bluetooth Wireless Communication.
- Industrial Grade Design - Isolated & Protected IO & EMC / EMI Compliance.
- Protocol JSON / MQTT, RESTful, TCP/UDP, SNMP & OPC.
- Support Secure Communication SSL.
- 16 GB SD Card Storage*.
- Support Most of the Cloud Platforms including Microsoft Azure & AWS etc.
- Real Time Clock - RTC DS3231, Accuracy: : +/- 3.5ppm From -40 to +85 Degree C.
- Power Supply - DC 9-36V.
- Controller / Processor : Quad Core 64 Bit ARM Cortex - A53 CPU 512 MB RAM.

### Benefiits

Cloud PLC® 4.0 can used to build the custom industrial solution for monitoring and controlling PLC and SCADA, HMI, VFD, Motors, servo, Valves, energy meter, actuators, relays, encoder, RFID and fingerprint readers and industrial sensors.

### Application

- Production and process monitoring.
- Utilities monitoring.
- Condition monitoring.
- Environment monitoring.
- Industrial Smart grid.

- Leakage detection.
- Generator monitoring.
- Cold storage monitoring.
- Industrial Smart grid.

- District Metering.
- Water Treatment.
- Green House.
- Warning message in case of calamities.

### Specification

#### Isolated Digital Inputs

- Number of Digital Inputs : 4
- Type of Digital Input : Isolated with Interrupted,
  WET / DRY connection supported
- Max Input Voltage Range : 0-24V
- Logic HIGH Trigger Voltage : > 12V
- Logic LOW Trigger Voltage : < 10V
- Maximum Trigger Frequency : 5Khz
- Protection of Digital Outputs : ESD, Transient

#### Isolated Digital Outputs

- Number of Digital Outputs : 4
- Type of Digital Output : Isolated / PWM
- Output Voltage Range : Open collector output 24V
- Maximum Current per Output : 100 mA
- Maximum Switching Frequency : 5Khz
- Protection of Digital Outputs : ESD, Transient

#### Isolated Analog input 0-24V

- Number of Analog Inputs : 4
- Type of Analog Inputs : Isolated 3700 Vrms
- Range of voltage measurement : 0-24V
- Resolution : 16 bit
- Protection of Analog Inputs : ESD, Transient

#### Isolated Input 4-20mA

- Number of 4-20mA Inputs : 4
- Type of 4-20mA Inputs : Isolated 3700 Vrms
- Range of current measurement : 4-20mA
- Resolution : 16 bit
- Protection of Analog inputs : ESD, Transient

#### Isolated Analog Output 0-10V

- Number of Analog Outputs : 2
- Type of Analog Outputs : Isolated 3700 Vrms
- Range of Voltage measurement : 0-10V
- Resolution : 16 bit
- Protection of Analog Inputs : ESD, Transient

#### Isolated Analog Output 4-20mA

- Number of 4-20mA Ouputs : 2
- Type of 4-20mA Ouputs : Isolated 3700 Vrms
- Range of current measurement : 4-20mA
- Resolution : 16 bit
- Protection of Analog inputs : ESD, Transient

#### Processor

Raspberry Pi Zero :

- SoC Name : BCM2835 | RAM : 512 MB
- Processor : Single-Core ARM1176JZF-S

Raspberry Pi Zero W :

- SoC Name : BCM2835 | RAM : 512 MB
- Processor : Single-Core ARM1176JZF-S

Raspberry Pi Zero 2W :

- SoC Name : RP3A0 | RAM : 512 MB
- Processor : Quad-core 64-bit Arm Cortex A53 CPU

#### Wireless Communication

- Wi-Fi : 802.11 b/g/n/e/I (802.11n @ up to 150 Mbit/s
- Bluetooth : V4.2 Bluetooth low Energy (BLE)
- Protocol : TCP / IP, JSON , MQTT , SSL , FTP, RESTful
- Security : WFA,WPA/WPA2 and WAPI

#### Wired Communication

Isolated RS485
- Isolation : 2500 Vrms
- Duplex type / Protocol : Half Duplex / MODBUS RTU
- Number of receivers on bus : 32
- Data rate : 115 Kbps
- Connector type : Screw Connector A, B, GND

#### USB

- Chipset : FTDI
- Baud rate : 115kbps
- Connector Type : USB B

#### Memory FRAM

- Memory : 448Kb
- On Chip SRAM : 520Kb
- RTC SRAM : 8Kb
- EEPROM : 4Kb
- Write Cycle : 1 Trillion

#### Relay

- No. of Relay : 2x
- Power Rating : 7A 250V AC, 12A 120V

#### Memory SD Card

- Memory : 8 to 32 GB
- DATA Storing Format : CSV

#### RTC - CR1220

- Battery Backup : 3.3V
- Accuracy : +/- 3.5ppm From -40 to +85 Degree C

#### Supply Voltage

- Supply Input Voltage : 12V / 24V
- Permissible range, Lower limit (DC) : 9V
- Permissible range, Upper limit (DC) : 36V

#### Installation

- Mounting : Wall / DIN Rail
- Enclosure : IP20

#### Dimensions

- Length : 110mm
- Height : 72.5mm
- Width : 110mm
- Weight : 150g