RDL743

# ARM Development Board LPC2148

LPC2148essential development features a plug and play design that makes it easy for connections and helps Students, hobbyists, enthusiasts, and professionals to focus more on Program / application development. LPC2148 Trainer Kit equipped with on board IO’s, communication interfaces & peripherals. It is really easy to design, experiment with, and test circuits without soldering. It’s used in many educational institutions and R&D LAB across the world.

### Features

- Plug & Play Interface Connectivity.
- Professional EMI/RFI Complaint PCB Layout Design.
- Modular Block design makes Easy access & quick Prototyping.
- FRC connectivity features minimize the connection Error.
- High Quality Grade PCB with wooden Enclosure.
- Stackable daughter board LPC2148.
- On board debugging JTAG Option
- USB onboard programming
- 8 interfacing LED’s.
- 1 * 4 interfacing keys.
- 4* 4 interfacing keypad matrix.
- Two channel RS232 port for communication.
- 3 ADC potentiometer input interface.
- 16X2 LCD, OLED interface.
- 46 general purpose IO
- On Board Power supply 3.3V, 5V 12V,GND.
- 8 pin DIP switches.
- On board voltage level converter
- Board enabled with the header for stacking the WiFi module.
- Board enabled with the header for stacking the Arduino shields.
- ON board Micro SD card
- RDL bus.
- External jumper nodes.
- Reset button.
- Power plug-in DC Socket.
- Power supply indicator LED.
- Test led for Tx, Rx.
- 7Seg Multiplexed Display.
- FT232RL USB communication.

### Note

Optional OLED & SDCARD modules are provided on this board, Hobbyists/developers can make use of this module with their previous knowledge or open-source community support and we do not have the support for the optional module.

### Scope of Learning Experiments:

- LED blinking.
- 8 bit LED Left shift, Right shift and counting operation.
- Keypad Interrupt Interface.
- 16*2 LCD interface.
- Matrix Keypad Interface.
- ADC & DAC interface.
- Traffic Light Signal Interface.
- 8 bit DIP switch interface.
- 7 Segment interface.
- L298 Driver for DC Motor and Stepper motor interface.
- Elevator Interface.
- Buzzer, Relay interface.
- RS485, RS232 serial communication.
- UART Operation.
- RTC DS1307I2C protocol interface.
- RF/WiFiCommunication.
- SPI protocol interface.
- Temperature Sensor Interface.
- Automatic Number Plate Recognition

### Package Contains:

- Development Board with Wooden Enclosure
- USB Cable.
- 12V 2A Adapter.
- FRC Cable