RDL740

# PIC Development Board

PIC essential development features a plug-and-play design that makes it easy for connections and helps Students, hobbyists, enthusiasts, and professionals to focus more on Program / application development. PIC Development Board Trainer kit equipped with on board IO’s, communication interfaces & peripherals. It is really easy to design, experiment with, and test circuits without soldering. It’sused in many educational institutions and R&D LAB across the world.

### Features

- Plug & Play Interface Connectivity.
- Professional EMI/RFI Complaint PCB Layout Design.
- Modular Block design makes Easy access & quick Prototyping.
- FRC connectivity features minimize the connection Error.
- High Quality Grade PCB with wooden Enclosure.
- On board Programming.
- 8 interfacing LED’s.
- 1*4 Menu keypad.
- 4*4 Matrix Keypad.
- RS232, RS485, USB communication port.
- 7 Segment Multiplexed Display.
- 16*2 LCD & OLED Display
- 8 bit 4 port IO.
- On Board WiFi / Bluetooth Connectivity.
- 3.3 to 5V Level Converter.
- Power Supply 3.3V and 5V.
- SD CARD Interface.
- RTC & EEPROM Interface.
- DC Motor/ Stepper Motor Driver.
- Relay, Buzzer.
- 1xTemperature Sensor.
- 3x Analog Test POT.

### Note

Optional OLED & SDCARD modules are provided on this board, Hobbyists/developers can make use of this module with their previous knowledge or open-source community support and we do not have the support for the optional module.

### MCU

- Only 35 single-word instructions to learn.
- All single-cycle instructions except for program branches, which are two-cycle.
- Operating speed: DC – 20 MHz clock input DC – 200 ns instruction cycle.
- Up to 8K x 14 words of Flash Program Memory, Up to 368 x 8 bytes of Data Memory (RAM), Up to 256 x 8 bytes of EEPROM Data Memory.
- Pinout compatible to other 28-pin or 40/44- pin PIC16CXXX and PIC16FXXX microcontrollers.

### Analog Features

- 10-bit, up to 8-channel Analog-to- Digital Converter(A/D).

### Peripheral Features

- Timer0: 8-bit timer/counter with 8-bit prescaler.
- Timer1: 16-bit timer/counter with prescaler.
- Timer2: 8-bit timer/counter with 8-bit period register,prescaler and postscaler.
- Two Capture, Compare, PWMmodules.
- Synchronous Serial Port (SSP) with SPI™ (Mastermode)and I2C™ (Master/Slave).
- Universal Synchronous Asynchronous Receiver Transmitter(USART/SCI) with 9-bit address detection.
- Parallel Slave Port (PSP) – 8 bits wide with external RD,WR and CS controls (40/44-pin only).

### Scope of Learning Experiments:

- LED blinking.
- 8 bit LED Left shift, Right shift and counting operation.
- Keypad Interrupt Interface.
- 16*2 LCD interface.
- Matrix Keypad Interface.
- ADC & DAC interface.
- Traffic Light Signal Interface.
- 8 bit DIP switch interface.
- 7 Segment interface.
- L298 Driver for DC Motor and Stepper motor interface.
- Elevator Interface.
- Buzzer, Relay interface.
- RS485, RS232 serial communication.
- PWM Interface.
- UART Operation.
- RTC DS1307I2C protocol interface.
- AT24C04 EEPROM I2C protocol interface.
- RF/WiFiCommunication.
- SPI protocol interface.
- Temperature Sensor Interface.

### Supported IC:

PIC16F74, PIC16F77, PIC16F747, PIC16F777, PIC16F871, PIC16F874, PIC16F877, PIC16F877A, PIC16F887, PIC18F452, PIC18F458, PIC18F4220, PIC18F4320, PIC18F4431, PIC18F4331, PIC18F4520, PIC18F4420, PIC18F4550, PIC18F4455, PIC18F4580, PIC18F4480, PIC18F4585, PIC18F4680, PIC18F4620, PIC18F45J10, PIC18F44J10, PIC18F44JPIC18F43K20, PIC18F44K20, PIC18F46K20

### Package Contains:

- Development Board with Wooden Enclosure
- USB Cable.
- 12V 2A Adapter.
- FRC Cable