RDL847

# 8051 Development Board

8051 essential development features a plug and plays design that makes it easy for connections and helps Students, hobbyists, enthusiasts, and professionals to focus more on Program/application development. 8051 Development Trainer kit equipped with onboard IO’s, communication interfaces & peripherals. It is really easy to design, experiment with, and test circuits without soldering. It’s used in many Educational Institutions and R&D LAB across the world.

### Features

- Plug & Play Interface Connectivity.
- Professional EMI/RFI Complaint PCB Layout Design.
- Modular Block design makes Easy access & quick Prototyping.
- FRC connectivity features minimize the connection Error.
- High Quality Grade PCB with wooden Enclosure.
- The DIP40 locking device for reuse ATMEL microcontroller.
- Supports 8051, AT89SXX and AT89CXX series chips 40 pin DIP package.
- On Board Programming
- 8 interfacing LED’s.
- 1 * 4 Menu keypad.
- 4* 4 Matrix Keypad.
- RS232, RS485, USB communication port.
- 16*2 LCD & OLED Display
- 8 bit 4 port IO.
- 3.3 to 5V Level Converter.
- Power Supply 3.3V and 5V
- SD CARD Interface.
- RTC & EEPROM Interface.
- DC Motor/ Stepper Motor Driver.
- Relay, Buzzer.
- 1xTemperature Sensor.
- 3x Analog Test POT.

### Note

Look into the datasheet for more details.
Optional OLED & SDCARD modules are provided on this board, Hobbyists/developers can make use of this module with their previous knowledge or open-source community support and we do not have the support for the optional module.

### Scope of Learning Experiments:

- LED blinking.
- 8 bit LED Left shift, Right shift and counting operation.
- Keypad Interrupt Interface.
- 16*2 LCD interface.
- Matrix Keypad Interface.
- ADC & DAC interface.
- Traffic Light Signal Interface.
- 8 bit DIP switch interface.
- 7 Segment interface.
- L298 Driver for DC Motor and Stepper motor interface.
- Elevator Interface.
- Buzzer, Relay interface.
- RS232 serial, RS485 and USB communication.
- UART Operation.
- RTC DS1307I2C protocol interface.
- AT24C04 EEPROM I2C protocol interface.
- RF/WiFi Communication.
- Temperature Sensor Interface.

### Package Includes:

- Development Board with Wooden Enclosure
- USB Cable.
- 12V 2A Adapter.